The attached Tcic program reads the board in the port specified at the maximal
available rate and produces a file with the specified name. The file includes all
the readings and finally the rate achieved.
Please note that the original Mscomm32.ocx supports only COM1 through COM16.
If you need a higher COM #, please replace the original Mscomm32.ocx (in the
folder \WINDOWS\system32) by the attached Mscomm32.ocx file.